Enable MQTT

Configure the following items under interfaces in config.json.

Open terminal and paste

sudo nano /home/pi/nodejs-poolController/config.json

"mqtt": {

"name": "MQTT",

"type": "mqtt",

"enabled": true"

"fileName": "mqtt.json",

"globals": {},

"options": {

"protocol": "mqtt://",

"host": "192.168.0.103",

"port": 1883,

"username": "",

"password": "",

"rootTopic": "pool",

"retain": true,

"qos": 0

Notes, change the following three items;

“true” enables MQTT client in poolController.

Host “IP” is the IP address of the MQTT broker ie. mcsMQTT,

RootTopic “pool” is used to sort mqtt topics.