Enable MQTT

Configure the following items under interfaces in config.json.

Open terminal and paste

sudo nano /home/pi/nodejs-poolController/config.json

"mqtt": {

 "name": "MQTT",

 "type": "mqtt",

 "enabled": true"

 "fileName": "mqtt.json",

 "globals": {},

 "options": {

 "protocol": "mqtt://",

 "host": "192.168.0.103",

 "port": 1883,

 "username": "",

 "password": "",

 "rootTopic": "pool",

 "retain": true,

 "qos": 0

Notes, change the following three items;

“true” enables MQTT client in poolController.

Host “IP” is the IP address of the MQTT broker ie. mcsMQTT,

RootTopic “pool” is used to sort mqtt topics.